|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Type | code | custom | electrode gap | gasket/seal | Interval | key dimensions | thread length | thread | recommended tightening torque | detail |
| AR08GS | 1515 | \* |  | P | max. 50 motohodin (Racing) | 16 mm | 19 mm | M 10x1,00 | 10-15 Nm |  |
| BR08GS |  | \* |  | P | max. 50 motohodin (Racing) | 16 mm | 19 mm | M 12x1,25 | 15-20 Nm |  |
| CR08GS | 1834 | \* |  | P | max. 50 motohodin (Racing) | 14 mm | 26,5 mm | M 10x1,00 | 10-15 Nm |  |
| DR08GS |  | \* |  | P | max. 50 motohodin (Racing) | 16 mm | 19 mm | M 14x1,25 | 20-30 Nm |  |
| ER10GS |  | \* |  | P | max. 50 motohodin (Racing) | 16 mm | 26,5 mm | M 14x1,25 | 20-30 Nm |  |